**Micro-Star International Co., Ltd.**

NO. 69, Lide St.,Zhonghe Dist.,

New Taipei City, TAIWAN, R.O.C.

TEL: 886-2-3234-5599 (REP)

FAX: 886-2-2225-0272



# Product Change Notice

# □Approval / ■Inform Sheet

# DATE: 2018/08/24

|  |  |  |  |
| --- | --- | --- | --- |
| **Model No.** | MS-98A9, MS-9899, MS-9887 | **PCN NO.** | IPC-20180824001 |
| **ERP No.** | 609-98A9-010/020/040/060,609-9899-050, 609-9887-030/040 | | |
| **Priority:** | □URGENT ■NORMAL | | |

|  |  |  |
| --- | --- | --- |
| **Change Type** | **Old** | **New** |
| □ PCB Change |  |  |
| □ H/W Component Change |  |  |
| □ BIOS change |  |  |
| □ Driver change |  |  |
| ■ Others: PCH | B01-00Q7735-I06  INTEL ( BD82Q77 ) | No AVL |
| B01-0HM7605-I06  INTEL (BD82HM76 ) | No AVL |
| B01-0HM6575-I06 INTEL (BD82HM65 ) | No AVL |
| B01-00Q6735-I06 INTEL ( BD82QM67 ) | No AVL |

|  |
| --- |
| **Problem Description:** |
| Intel announced Sandy Bridge, Ivy Bridge EOL. |
| **Explanation:**  Intel announced Sandy Bridge, Ivy Bridge PCH will be discontinued.   |  | | --- | | **Intel PCN** | |  |   **Impact Model:**   |  |  |  |  | | --- | --- | --- | --- | | **Model** | **ERP** | **MSI PN** | **Intel PN** | | 98A9 | 609-98A9-010 | B01-00Q7735-I06 | BD82Q77 | | 609-98A9-020 | | 609-98A9-040 | | 609-98A9-060 | | 9899 | 609-9899-050 | B01-0HM7605-I06 | BD82HM76 | | 9887 | 609-9887-040 | B01-0HM6575-I06 | BD82HM65 | | 609-9887-030 | B01-0QM6715-I06 | BD82QM67 |   **Forecasted Key Milestones:** |

|  |
| --- |
| **ECN Inform Sheet :** |
| **Customer’s Reply:** |
| □ Accept |
| □ Do not accept |
| **Production Instruction:** |
| □ Cut in Immediately □ Running Change □ RMA Cut in |
| **Explanation, Comments and Suggestions:** |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Issued By** | Jennifer | Reviewed By | Arthur |

**Counter signature**

■ N/A

□Please sign this form and fax back not later than . If no confirmation or rejection has been received from you after the said date, we will assume your acceptance and implement the modifications.